. |  | Balik | Lanjut

# Graphical Configuration

### Graphics Card and Monitor Configuration

No matter which graphical environment (also known as desktop environment) you chose for this install of Mageia, they are all based on a graphical user interface system called `X Window System`, or simply “X”. So in order for KDE Plasma, GNOME, LXDE or any other graphical environment to work well, the following “X” settings need to be correct.

Choose the appropriate settings manually if you think the details are incorrect, or if none are shown.

- Graphics Card

  If you need to, you can select a specific card from this expandable list. See Pilih Server X (Konfigurasi Perangkat Grafis Anda).

- Monitor

  You can choose Plug 'n Play, if applicable, or choose your monitor from the Vendor or Generic lists. Choose Custom if you prefer to manually set the horizontal and vertical refresh rates of your monitor. See Pemilihan Monitor.

- Resolution

  The resolution and color depth of your monitor can be set here.

- Test

  The test button does not always appear during install. If the option is there, and you test your settings, you should be asked to confirm that your settings are correct. If you answer Yes, the settings will be kept. If you don't see anything, you'll return to the configuration screen and be able to reconfigure everything until the test result is satisfactory. If the test option is not available, then make sure your settings are on the safe side.

- Options

  Here you can choose to enable or disable various options.

### Awas

There is a risk of damaging a monitor if you choose refresh rates that are outside the frequency range of that monitor. This applies to older CRT displays: modern monitors will reject an unsupported frequency and normally enter standby mode.

### Pilih Server X (Konfigurasi Perangkat Grafis Anda)

DrakX memiliki basis data perangkat video yang lengkap dan biasanya akan mengidentifikasi perangkat video Anda dengan benar.

Jika installer tidak mendeteksi perangkat grafis Anda dengan benar dan Anda mengetahui mana yang Anda punya, Anda bisa memilihnya dari pohon dengan:

- Vendor

- then the make of your card

- and the model of card

If you cannot find your card in the vendor lists (because it's not yet in the database or it's an older card) you may find a suitable driver in the Xorg category, which provides more than 40 generic and open source video card drivers. If you still can't find a specific driver for your card there is the option of using the VESA driver which provides basic capabilities.

### Perhatian

Be aware that if you select an incompatible driver you may only have access to the Command Line Interface

Some video card manufacturers provide proprietary drivers for Linux which may only be available in the Nonfree repository and in some cases only from the card manufacturers' websites. The Nonfree repository needs to be explicitly enabled to access them. If you didn't enable it previously, you should do this after your first reboot.

### Pemilihan Monitor

DrakX memiliki basis data monitor yang lengkap dan biasanya akan mengenali monitor Anda dengan tepat.

### Awas

Selecting a monitor with different characteristics could damage your monitor or video hardware. Please don't try something without knowing what you are doing. If in doubt you should consult your monitor documentation.

Sesuaian

  This option allows you to set two critical parameters: the vertical refresh rate and the horizontal sync rate. Vertical refresh determines how often the screen is refreshed and horizontal sync is the rate at which scan lines are displayed.

  SANGAT PENTING untuk tidak menentukan tipe monitor dengan jarak sync diluar kemampuan monitor: Anda bisa merusak monitor. Jika ragu, pilih pengaturan sederhana dan baca dokumentasi monitor yang Anda miliki.

Plug'n Play

  This is the default option and automatically tries to determine the monitor type from the monitor database.

Vendor

  If the installer has not correctly detected your monitor and you know which one you have, you can choose it from the options by selecting:

- Manufacturer

- Monitor model

Generik

  Selecting this group will list approximately 30 display configurations such as 1024x768 @ 60Hz and includes flat-panel displays as used in laptops. This is often a good monitor selection group if you need to use the VESA card driver when your video hardware cannot be determined automatically. Once again, it may be wise to be conservative in your selections.

© Mageia
CC BY-SA 3.0

Balik |  | Lanjut
| Depan |

- Contents
- Search

- Pilih dan gunakan ISO
  - Pengantar
  - Media
    - Definisi
    - Media instalasi klasik
      - Fitur umum
    - Media live
      - Fitur umum
      - Live DVD Plasma
      - Live DVD GNOME
      - Live DVD Xfce
    - Net install media
      - Fitur umum
      - netinstall.iso
      - netinstall-nonfree.iso
  - Mengunduh dan Memeriksa Media
    - Mengunduh
    - Checking the integrity of the downloaded media
  - Bakar atau salin ISO
    - Membakar ISO ke CD/DVD
    - Salin ISO ke flashdisk
      - Using a graphical tool within Mageia
      - Using a graphical tool within Windows
      - Using the Command line within a GNU/Linux system
- DrakX, Installer Mageia
  - Langkah-langkah instalasi
  - Layar Selamat Datang untuk Instalasi
    - Legacy (BIOS) Systems
    - UEFI Systems
  - Masalah Instalasi dan Kemungkinan Solusinya
    - Tidak Ada Antarmuka Grafis
    - Instalasi Membeku
    - Masalah RAM
    - Partisi dinamis
- Silakan pilih bahasa yang akan digunakan
- Lisensi dan Catatan Rilis
  - Perjanjian Lisensi
  - Catatan Rilis
- Pengaturan SCSI
- Install atau Upgrade
- Konfigurasi Zona Waktu Anda
- Date, Clock and Time Zone Settings
- Keyboard
- Pemartisian
  - Suggested Partitioning
  - Pilih titik kait
  - Konfirmasi harddisk yang akan diformat
  - Custom Disk Partitioning with DiskDrake
  - Pemformatan
- Software
  - Pemilihan Media
    - Supplemental Installation Media
    - Available Media
  - Pemilihan Desktop
  - Pemilihan Grup Paket
  - Instalasi Minimal
  - Pilih Paket Individual
- User Management
  - Atur Sandi Administrator (root):
  - Masukkan pengguna
  - User Management (advanced)
- Graphical Configuration
  - Graphics Card and Monitor Configuration
  - Pilih Server X (Konfigurasi Perangkat Grafis Anda)
  - Pemilihan Monitor
- Bootloader
  - Available Bootloaders
    - Grub2
    - rEFInd
  - Bootloader Setup
    - Pilihan utama Bootloader
    - Konfigurasi Bootloader
  - Opsi Lain
    - Gunakan bootloader yang ada
    - Installing Without a Bootloader
    - Tambah atau Modifikasi Entri Menu Boot
- Configuration Summary
  - Parameter sistem
  - Parameter hardware
  - Parameter Jaringan dan Internet
  - Keamanan
- Pilih Negara / Wilayah Anda
  - Metode masukan
- Konfigurasikan Layanan Anda
- Pilih mouse
- Konfigurasi Suara
  - Lanjutan
- Tingkat Keamanan
- Firewall
- Update
- Selamat
- Uninstall Mageia

Search