. |  | Poprzedni | Następny

# Graphical Configuration

### Graphics Card and Monitor Configuration

No matter which graphical environment (also known as desktop environment) you chose for this install of Mageia, they are all based on a graphical user interface system called `X Window System`, or simply „X”. So in order for KDE Plasma, GNOME, LXDE or any other graphical environment to work well, the following „X” settings need to be correct.

Choose the appropriate settings manually if you think the details are incorrect, or if none are shown.

- Graphics Card

  If you need to, you can select a specific card from this expandable list. See Wybierz System Graficzny (Skonfiguruj swoją Kartę Graficzną).

- Monitor

  You can choose Plug 'n Play, if applicable, or choose your monitor from the Vendor or Generic lists. Choose Custom if you prefer to manually set the horizontal and vertical refresh rates of your monitor. See Wybór monitora.

- Resolution

  The resolution and color depth of your monitor can be set here.

- Test

  The test button does not always appear during install. If the option is there, and you test your settings, you should be asked to confirm that your settings are correct. If you answer Yes, the settings will be kept. If you don't see anything, you'll return to the configuration screen and be able to reconfigure everything until the test result is satisfactory. If the test option is not available, then make sure your settings are on the safe side.

- Options

  Here you can choose to enable or disable various options.

### Ostrzeżenie

There is a risk of damaging a monitor if you choose refresh rates that are outside the frequency range of that monitor. This applies to older CRT displays: modern monitors will reject an unsupported frequency and normally enter standby mode.

### Wybierz System Graficzny (Skonfiguruj swoją Kartę Graficzną)

DrakX posiada bardzo szeroką bazę danych kart wideo, oraz zwykle zidentyfikuje twoje urządzenie wideo poprawnie.

Jeżeli instalator nie wykrył twojej karty graficznej poprawnie i wiesz, jaką kartę posiadasz, możesz wybrać jedną za pomocą:

- Dostawca

- then the make of your card

- and the model of card

If you cannot find your card in the vendor lists (because it's not yet in the database or it's an older card) you may find a suitable driver in the Xorg category, which provides more than 40 generic and open source video card drivers. If you still can't find a specific driver for your card there is the option of using the VESA driver which provides basic capabilities.

### Uwaga!

Be aware that if you select an incompatible driver you may only have access to the Command Line Interface

Some video card manufacturers provide proprietary drivers for Linux which may only be available in the Nonfree repository and in some cases only from the card manufacturers' websites. The Nonfree repository needs to be explicitly enabled to access them. If you didn't enable it previously, you should do this after your first reboot.

### Wybór monitora

DrakX has a very comprehensive database of monitors and will usually correctly identify yours.

### Ostrzeżenie

Selecting a monitor with different characteristics could damage your monitor or video hardware. Please don't try something without knowing what you are doing. If in doubt you should consult your monitor documentation.

Własne

  This option allows you to set two critical parameters: the vertical refresh rate and the horizontal sync rate. Vertical refresh determines how often the screen is refreshed and horizontal sync is the rate at which scan lines are displayed.

  It is VERY IMPORTANT that you do not specify a monitor type with a sync range that is beyond the capabilities of your monitor: you may damage your monitor. If in doubt, choose a conservative setting and consult your monitor documentation.

Plug'n Play

  This is the default option and automatically tries to determine the monitor type from the monitor database.

Dostawca

  If the installer has not correctly detected your monitor and you know which one you have, you can choose it from the options by selecting:

- Manufacturer

- Monitor model

Standardowa

  Selecting this group will list approximately 30 display configurations such as 1024x768 @ 60Hz and includes flat-panel displays as used in laptops. This is often a good monitor selection group if you need to use the VESA card driver when your video hardware cannot be determined automatically. Once again, it may be wise to be conservative in your selections.

© Mageia
CC BY-SA 3.0

Poprzedni |  | Następny
| Spis treści |

- Contents
- Search

- Wybierz i użyj obrazu ISO
  - Wprowadzenie
  - Nośnik
    - Definicja
    - Klasyczne medium instalacji
      - Powszechne możliwości
    - Nośniki live
      - Powszechne możliwości
      - Live DVD Plasma
      - Live DVD GNOME
      - Live DVD Xfce
    - Net install media
      - Powszechne możliwości
      - netinstall.iso
      - netinstall-nonfree.iso
  - Pobieranie i Sprawdzanie Mediów
    - Pobieranie
    - Checking the integrity of the downloaded media
  - Wypal lub zrzuć obraz ISO
    - Wypalenie obrazu ISO na CD/DVD
    - Zrzuć obraz ISO na pamięci USB
      - Używanie graficznych narzędzi w Magei
      - Używanie graficznych narzędzi w Windows
      - Using the Command line within a GNU/Linux system
- DrakX instalator Mageia
  - Etapy instalacji
  - Ekran powitalny instalatora
    - Legacy (BIOS) Systems
    - UEFI Systems
  - Problemy z instalacją oraz możliwe rozwiązania
    - Brak graficznego interfejsu
    - Zawieszenie się instalacji
    - Problem z pamięcią RAM
    - Dynamiczne partycje
- Wybór języka
- Licencja oraz informacje o wydaniu
  - Umowa Licencyjna
  - Informacje o Wydaniu
- Wykrywanie SCSI
- Instalacja czy uaktualnienie
- Konfiguruj strefę czasową
- Date, Clock and Time Zone Settings
- Klawiatura
- Partycjonowanie
  - Suggested Partitioning
  - Wybierz punkty montowania
  - Formatowanie twardego dysku
  - Custom Disk Partitioning with DiskDrake
  - Formatowanie
- Software
  - Wybór nośników
    - Supplemental Installation Media
    - Available Media
  - Wybór pulpitu
  - Wybór grup pakietów
  - Minimalna instalacja
  - Samodzielny wybór pakietów
- User Management
  - Ustawienie hasła administratora (root):
  - Dodaj użytkownika
  - User Management (advanced)
- Graphical Configuration
  - Graphics Card and Monitor Configuration
  - Wybierz System Graficzny (Skonfiguruj swoją Kartę Graficzną)
  - Wybór monitora
- Program rozruchowy
  - Available Bootloaders
    - Grub2
    - rEFInd
  - Bootloader Setup
    - Podstawowe opcje programu rozruchowego
    - Konfiguracja programu rozruchowego
  - Inne opcje
    - Użyj istniejącego bootloader'a.
    - Installing Without a Bootloader
    - Dodaj lub zmodyfikuj wpis Boot Menu
- Configuration Summary
  - Parametry systemu
  - Parametry sprzętu
  - Network and Internet parameters
  - Bezpieczeństwo
- Wybierz twój Kraj / Region
  - Metoda wejścia
- Konfiguracja usług
- Wybierz mysz
- Konfiguracja dźwięku
  - Zaawansowane
- Poziom bezpieczeństwa
- Zapora sieciowa
- Aktualizacje
- Gratulacje
- Usuwanie Magei

Search