. |  | Nazaj | Naprej

# Zagonski nalagalnik

### Available Bootloaders

#### Grub2

Grub2 on Legacy MBR/GPT systems

- GRUB2 (with or without graphical menu) will be used exclusively as the bootloader for a Legacy/MBR or Legacy/GPT system.

- By default, a new bootloader will be written into either the MBR (Master Boot Record) of your first hard drive or in the BIOS boot partition.

Grub2-efi on UEFI systems

- GRUB2-efi or rEFInd may be used as the bootloader for a UEFI system.

- By default, a new bootloader (Grub2-efi) will be written into the ESP (EFI System Partition).

  If there are already UEFI-based operating systems installed on your computer (Windows 8 for example), the Mageia installer will detect the existing ESP created by Windows and add grub2-efi to it. If no ESP exists, then one will be created. Although it is possible to have several ESPs, only one is required, whatever the number of operating systems you have.

#### rEFInd

rEFInd on UEFI systems

- rEFInd has a nice graphical set of options, and can auto-detect installed EFI bootloaders. See: http://www.rodsbooks.com/refind/

### Opomba

Please note that in order to be able to use the `rEFInd` option, an installed EFI System Partition must match your system architecture: if you have a 32bit EFI System Partition installed on a 64bit machine for instance, then the rEFInd option will not be displayed/available to you.

### Bootloader Setup

#### Glavne možnosti zagonskega nalagalnika

- Bootloader to use

  - GRUB2 (with either a graphical or a text menu), can be chosen for both `Legacy MBR/BIOS` systems and `UEFI` systems.

  - rEFInd (with a graphical menu) is an alternative option solely for use with `UEFI` systems.

- Boot device

  ### Pozor

  Don't change this unless you really know what you are doing.

  ### Opomba

  There is no option to write GRUB to the boot sector of a partition (e.g: `sda1`), as this method is considered unreliable.

  When using UEFI mode, then the Boot device will be listed as EFI System Partition.

- Delay before booting the default image

  This text box lets you set a delay, in seconds, before the default operating system is started up.

- Security

  This allows you to set a password for the bootloader. This means a username and password will be required when booting in order to select a booting entry or change settings. This is optional, and most people are not likely to have a need for it. The username is `root` and the password is the one chosen hereafter.

- Password

  Choose a password for the bootloader (optional)

- Password (again)

  Retype the password and DrakX will check that it matches with the one set above

Advanced

- Enable ACPI

  ACPI (Advanced Configuration and Power Interface) is a standard for power management. It can save energy by stopping unused devices. Deselecting it could be useful if, for example, your computer does not support ACPI or if you think the ACPI implementation might cause some problems (for instance random reboots or system lockups).

- Enable SMP

  This option enables/disables symmetric multiprocessing for multi-core processors

- Enable APIC

  Enabling this gives the operating system access to the Advanced Programmable Interrupt Controller. APIC devices permit more complex priority models, and Advanced IRQ (Interrupt Request) management.

- Enable Local APIC

  Here you can set Local APIC, which manages all external interrupts for a specific processor in an SMP system

#### Nastavitev zagonskega nalagalnika

If, in the previous section you selected `rEFInd` as the bootloader to use, you would then be presented with the options shown in the screenshot directly below. Otherwise, please instead move on to the subsequent screenshot for your options.

Your rEFInd configuration options:

- Install or update rEFInd in the EFI system partition.

- Install in /EFI/BOOT.

  This option installs the bootloader in the /EFI/BOOT directory of the ESP (EFI System Partition). This can be useful when:

  (a) Installing onto a removable drive (e.g. a USB stick) that can be removed and plugged into a different machine. If the bootloader is stored in /EFI/BOOT, UEFI BIOS's will detect it and allow you to boot from that drive.

  (b) As a workaround where, due to a buggy UEFI BIOS, the newly written bootloader for Mageia will not be recognized at end of the installation.

If you did not select rEFInd as the bootloader to use in the previous section, then your bootloader configuration options are shown below:

- Default

  The operating system to be started up by default.

- Append

  This option lets you pass information to the kernel or tell the kernel to give you more information as it boots.

- Probe foreign OS

  If you already have other operating systems installed, Mageia attempts to add them to your new Mageia boot menu. If you don't want this behaviour, then untick the Probe Foreign OS option.

- Install in /EFI/BOOT. (Note: this menu option only becomes available where the installer detects that a machine is in UEFI mode).

  This option installs the bootloader in the /EFI/BOOT directory of the ESP (EFI System Partition). This can be useful when:

  (a) Installing onto a removable drive (e.g. a USB stick) that can be removed and plugged into a different machine. If the bootloader is stored in /EFI/BOOT, UEFI BIOS's will detect it and allow you to boot from that drive.

  (b) As a workaround where, due to a buggy UEFI BIOS, the newly written bootloader for Mageia will not be recognized at end of the installation.

Advanced

- Video mode

  This sets the screen size and colour depth to be used by the boot menu. If you click the down-triangle you will be offered other size and colour depth options.

- Do not touch ESP or MBR

  Select this option if you don't want a bootable Mageia, but would rather chain-load it from another OS. You will get a warning that the bootloader is missing. Click Ok only if you are sure you understand the implications, and wish to proceed.

  ### Pozor

  Chain-loading via legacy bootloaders (GRUB Legacy and LiLo) is no longer supported by Mageia as it is likely to fail when attempting to boot this resulting installation of Mageia. If you use anything other than GRUB2 or rEFInd for this purpose, then you do so at your own risk!

### Druge možnosti

#### Uporaba obstoječega zagonskega nalagalnika

The exact procedure for adding Mageia to an existing bootloader is beyond the scope of this documentation. However, in most cases it will involve running the relevant bootloader installation program, which should detect Mageia and automatically add an entry for it in the bootloader menu. See the documentation for the relevant operating system.

#### Installing Without a Bootloader

While you can opt to install Mageia without a bootloader (see section 2.1 Advanced), this is not recommended unless you absolutely know what you are doing, as without some form of bootloader your operating system will be unable to start.

#### Add or Modify a Boot Menu Entry

To do this you need to manually edit /boot/grub2/custom.cfg or use the software grub-customizer tool instead (available in the Mageia repositories).

### Opomba

For more information, see: https://wiki.mageia.org/en/Grub2-efi_and_Mageia

© Mageia
CC BY-SA 3.0

Nazaj |  | Naprej
| Domov |

- Contents
- Search

- Izbor in uporaba odtisa diska: ISO
  - Predstavitev
  - Vir
    - Definicija
    - Mediji za klasično namestitev
      - Skupne značilnosti
    - Živi medij
      - Skupne značilnosti
      - Živi Plasma DVD
      - Živi GNOME DVD
      - Živi Xfce DVD
    - Net install media
      - Skupne značilnosti
      - netinstall.iso
      - netinstall-nonfree.iso
  - Downloading and Checking Media
    - Prejemanje
    - Checking the integrity of the downloaded media
  - Zapecite ali prenesite odtis diska
    - Burning the ISO to a CD/DVD
    - Odlaganje odtisa nosilca za namestitev na ključek USB
      - Using a graphical tool within Mageia
      - Using a graphical tool within Windows
      - Using the Command line within a GNU/Linux system
- DrakX, namestitveni program Mageje
  - Namestitveni koraki
  - Prikaz dobrodošlice namestitve
    - Legacy (BIOS) Systems
    - UEFI Systems
  - Težave z namestitvijo in možne rešitve
    - Brez grafičnega vmesnika
    - Namestitev zamrzne
    - Težave s spominom RAM
    - Dinamični razdelki
- Izberite jezik namestitve
- Licenčna pogodba in opombe ob izdaji
  - Licenčna pogodba
  - Opombe ob izdaji
- Nastavitev naprav SCSI
- Namestitev ali nadgradnja
- Nastavite vaš časovni pas
- Date, Clock and Time Zone Settings
- Tipkovnica
- Razdelitev diska
  - Predlagana razdelitev diska
  - Izberite priklopne točke
  - Potrdi formatiranje trdega diska
  - Razdeljevanje diska po meri s programom DiskDrake
  - Formatiranje
- Software
  - Izbira virov
    - Supplemental Installation Media
    - Available Media
  - Izbira namizja
  - Izbira skupin paketov
  - Minimalna namestitev
  - Izbira posamičnih paketov
- Upravljanje z uporabniki
  - Nastavite geslo skrbnika (uporabnika root):
  - Dodajte uporabnika
  - Upravljanje z uporabniki (napredno)
- Graphical Configuration
  - Nastavitev grafične kartice in monitorja
  - Izberite strežnik X ()nastavite grafično kartico
  - Izberite vaš zaslon
- Zagonski nalagalnik
  - Available Bootloaders
    - Grub2
    - rEFInd
  - Bootloader Setup
    - Glavne možnosti zagonskega nalagalnika
    - Nastavitev zagonskega nalagalnika
  - Druge možnosti
    - Uporaba obstoječega zagonskega nalagalnika
    - Installing Without a Bootloader
    - Add or Modify a Boot Menu Entry
- Configuration Summary
  - Sistemske nastavitve
  - Strojne nastavitve
  - Nastavitve omrežja in interneta
  - Varnost
- Izbor države/regije
  - Način vnosa
- Nastavite vaše storitve
- Izberite miško
- Nastavitve zvoka
  - Napredno
- Stopnja varnosti
- Požarni zid
- Posodobitve
- Čestitke
- Odstrani Magejo

Search