. |  | Önceki | Sonraki

# Graphical Configuration

### Graphics Card and Monitor Configuration

No matter which graphical environment (also known as desktop environment) you chose for this install of Mageia, they are all based on a graphical user interface system called `X Window System`, or simply “X”. So in order for KDE Plasma, GNOME, LXDE or any other graphical environment to work well, the following “X” settings need to be correct.

Choose the appropriate settings manually if you think the details are incorrect, or if none are shown.

- Graphics Card

  If you need to, you can select a specific card from this expandable list. See Bir X Sunucusu Seçme (Ekran Kartını Yapılandırma).

- Monitor

  You can choose Plug 'n Play, if applicable, or choose your monitor from the Vendor or Generic lists. Choose Custom if you prefer to manually set the horizontal and vertical refresh rates of your monitor. See Monitör Seçimi.

- Resolution

  The resolution and color depth of your monitor can be set here.

- Test

  The test button does not always appear during install. If the option is there, and you test your settings, you should be asked to confirm that your settings are correct. If you answer Yes, the settings will be kept. If you don't see anything, you'll return to the configuration screen and be able to reconfigure everything until the test result is satisfactory. If the test option is not available, then make sure your settings are on the safe side.

- Options

  Here you can choose to enable or disable various options.

### Uyarı

There is a risk of damaging a monitor if you choose refresh rates that are outside the frequency range of that monitor. This applies to older CRT displays: modern monitors will reject an unsupported frequency and normally enter standby mode.

### Bir X Sunucusu Seçme (Ekran Kartını Yapılandırma)

DrakX; ekran kartlarının karşılaştırmalı veritabanına sahip olup genellikle ekran kartınızı doğru olarak tanımlar.

Kurulum aracı ekran kartınızı doğru olarak algılayamamışsa ve kartınızın hangisi olduğunu biliyorsanız, kartınızı ağaçtan şuna göre seçebilirsiniz:

- Üretici

- then the make of your card

- and the model of card

If you cannot find your card in the vendor lists (because it's not yet in the database or it's an older card) you may find a suitable driver in the Xorg category, which provides more than 40 generic and open source video card drivers. If you still can't find a specific driver for your card there is the option of using the VESA driver which provides basic capabilities.

### Dikkat

Be aware that if you select an incompatible driver you may only have access to the Command Line Interface

Some video card manufacturers provide proprietary drivers for Linux which may only be available in the Nonfree repository and in some cases only from the card manufacturers' websites. The Nonfree repository needs to be explicitly enabled to access them. If you didn't enable it previously, you should do this after your first reboot.

### Monitör Seçimi

DrakX monitörlerin karşılaştırmalı veritabanına sahip olup genellikle monitörünüzü doğru olarak tanımlar.

### Uyarı

Selecting a monitor with different characteristics could damage your monitor or video hardware. Please don't try something without knowing what you are doing. If in doubt you should consult your monitor documentation.

Özel

  This option allows you to set two critical parameters: the vertical refresh rate and the horizontal sync rate. Vertical refresh determines how often the screen is refreshed and horizontal sync is the rate at which scan lines are displayed.

  Monitörünüzün kapasitesinin ötesinde bir monitör türü ve ekran aralığı belirlememeniz ÇOK ÖNEMLİDİR: monitörünüze zarar verebilirsiniz. Kararsız kalırsanız, ortalama bir ayar seçin ve monitörünüzün kılavuzuna bakın.

Tak ve Kullan

  This is the default option and automatically tries to determine the monitor type from the monitor database.

Üretici

  If the installer has not correctly detected your monitor and you know which one you have, you can choose it from the options by selecting:

- Manufacturer

- Monitor model

Genel

  Selecting this group will list approximately 30 display configurations such as 1024x768 @ 60Hz and includes flat-panel displays as used in laptops. This is often a good monitor selection group if you need to use the VESA card driver when your video hardware cannot be determined automatically. Once again, it may be wise to be conservative in your selections.

© Mageia
CC BY-SA 3.0

Önceki |  | Sonraki
| Başlangıç |

- Contents
- Search

- ISO'ları seçin ve kullanın
  - Giriş
  - Ortam
    - Açıklama
    - Klasik kurulum ortamı
      - Ortak özellikler
    - Canlı Ortam
      - Ortak özellikler
      - Canlı DVD Plasma
      - Canlı DVD GNOME
      - Canlı DVD Xfce
    - Net install media
      - Ortak özellikler
      - netinstall.iso
      - netinstall-nonfree.iso
  - Ortamları indirme ve kontrol etme
    - İndirme
    - İndirilen ortamın bütünlüğünü kontrol etme
  - ISO yakma veya atma
    - Bir CD/DVD üzerine ISO yakma
    - Bir USB bellek üzerine ISO atmak
      - Mageia üzerinde bir grafiksel araç kullanarak
      - Windows üzerinde bir grafiksel araç kullanarak
      - Using the Command line within a GNU/Linux system
- DrakX, Mageia Kurulum Aracı
  - Kurulum adımları
  - Kurulum Karşılama Ekranı
    - Legacy (BIOS) Systems
    - UEFI Systems
  - Kurulum Sorunları ve Muhtemel Çözümleri
    - Grafiksel Arabirim Yok
    - Kurulum Donuyor
    - RAM sorunu
    - Dinamik bölümler
- Lütfen kullanacağınız dili seçiniz
- Lisans ve Sürüm Notları
  - Lisans Sözleşmesi
  - Sürüm Notları
- SCSI Kur
- Kurulum veya Yükseltme
- Zaman Dilimini Yapılandırma
- Date, Clock and Time Zone Settings
- Klavye
- Bölümlendirme
  - Suggested Partitioning
  - Bağlama noktasını seçin
  - Biçimlendirilecek sabit diski onaylayın
  - Custom Disk Partitioning with DiskDrake
  - Biçimlendirme
- Software
  - Paket Grubu Seçimi
    - Supplemental Installation Media
    - Available Media
  - Masaüstü Seçimi
  - Paket Grubu Seçimi
  - En Ufak Kurulum
  - Paketleri Tek Tek Seçin
- User Management
  - Yönetici (kök) Parolasını Ayarlayın:
  - Bir kullanıcı girin
  - User Management (advanced)
- Graphical Configuration
  - Graphics Card and Monitor Configuration
  - Bir X Sunucusu Seçme (Ekran Kartını Yapılandırma)
  - Monitör Seçimi
- Önyükleyici
  - Available Bootloaders
    - Grub2
    - rEFInd
  - Bootloader Setup
    - Önyükleyici ana seçenekleri
    - Önyükleme Yapılandırması
  - Diğer Seçenekler
    - Mevcut bir önyükleyiciyi kullanmak
    - Installing Without a Bootloader
    - Önyükleme Menü Girdisi Ekleme veya Değiştirme
- Configuration Summary
  - Sistem parametreleri
  - Donanım parametreleri
  - Ağ ve İnternet parametreleri
  - Güvenlik
- Ülke/Bölge seçin
  - Girdi yöntemi:
- Hizmetleri Yapılandırma
- Fare seçin
- Ses Yapılandırması
  - Gelişmiş
- Güvenlik Seviyesi
- Güvenlik duvarı
- Güncellemeler
- Tebrikler
- Mageia' yı Kaldırma

Search